|  |  |  |
| --- | --- | --- |
| **Annex 1 to the Contract pursuant to DE-UZ 35**  **Blue Angel Eco-Label**  **„Wallpapers and Woodchip Wallpapers made primarily from Recycled Paper“** |  | **Please use this  form !** |

Manufacturer (Applicant):

- full address

Distributor (Label user):

- full address

Brand /trade name:

Product designation:   
according to paragraph 2

Wallpaper according to DIN 6730

Woodchip wallpaper according to DIN 6730

Virgin fibres and waste paper grades according to Appendix to DE-UZ 35 used in the product - leaving the incorporated wood fibres out of account:

|  |  |
| --- | --- |
| Survey A | |
| Fraction of fibrous material | Quantities used  per 1000 kg of manufactured new paper  (weight air dried) in kg |
| Ordinary grades  (Group 1) |  |
| Medium grades  (Group 2) |  |
| High grades  (Group 3) |  |
| Kraft Grades  (Group 4) |  |
| Special grades (Group 5) |  |
| Virgin fibres |  |

**Substances used in the manufacture of the product;**

**paras. 3.5, 3.6 and 3.7**

- The following substances are used in the manufacture (please mark where applicable);  
  
**Colorant**   Annexes 2 and 3 are attached

**Surface finishing agent**  Annex 3 to the Contract is attached

**Coating material**  Annex 3 to the Contract is attached

**none**

Bleaching agents and complexing agents used in the finished product in accordance with para. 3.8:

|  |  |  |
| --- | --- | --- |
| Survey B | | |
| Fibre processing | Bleaching agents  used | Complexing agents used |
| Waste paper  Virgin fibre |  |  |

Applicant’s Declarations:

|  |  |  |
| --- | --- | --- |
| **Paragraph** | It is hereby declared | **Yes** |
| **3.1.1** | - that the wallpaper contains a minimum of 600 kg of waste paper per 1000 kg of manufactured new paper (weight air dried),  - that at least 50 percent of these 600 kg consist of ordinary, medium and kraft waste papers, except for the individual grade 4.07, |  |
| **3.1.2** | - that woodchip wallpapers consist of 100 percent waste paper,  - that at least 50 percent thereof consist of ordinary and medium waste papers. |  |
| **3.2** | - that the wallpapers are manufactured without using chemical auxiliary agents that contain glyoxal or formaldehyde as constituents or can split off formaldehyde. |  |
| **3.3** | - that the content of releasable formaldehyde in the finished product does not exceed 8 mg/100 g of absolutely dry wallpaper,  - that the test protocol of an independent testing laboratory is attached hereto, |  |
| **3.4** | - that only those substances are used as biocides which have been approved under the Biocidal Products Regulation - Regulation (EU) No 528/2012 - (EU List of approved active substances; formerly inclusion in Annex I of the Biocidal Products Directive 98/09 EC) or which are still being reviewed as notified existing active substances for the respective type of biocidal product under the EU Review Programme for Existing Active Substances,  - that only those substances are used as biocidal products which have been approved for the respective field of use,  - that products containing existing active substances which are still under EU review may continue to be used without authorisation until a decision is reached,  - that, in addition, the products do not contain active substances considered as candidates for substitution in accordance with Article 10 of the Biocidal Products Regulation (EU) 528/2012,  - that pending the respective entry into force of the approval requirement for the use of biocidal products containing existing active substances only those substances may be used which are additionally listed in the 36th Recommendation of BfR (Federal Institute for Risk Assessment),  - that neither tetramethylthiuram disulfide (CAS No 127-36-8) nor nanosilver (CAS No 7440-22-4)  is used,  - that  - sodium hexafluorosilicate - CAS No 16893-85-9  - N-[α-(1-nitroethyl)benzyl] ethylenediamine CAS No 14762-38-0  - - mixture of tris-(hydroxymethyl)-nitromethane   CAS No 126-11-4,  - 5-chloro-2-methyl-4-isothiazolin-3-one CAS No 26172-55-4  and 2-methyl-4-isothiazolin-3-one CAS No 2682-20-4,  - tetramethylthiuram disulfide CAS No 127-36-8  - nanosilver CAS No 7440-22-4  are not used. |  |
| **3.8** | - that waste paper is processed without using any chlorine, halogenated bleaching agents and not readily biodegradable complexing agents, such as ethylenediaminetetraacetic acid (EDTA) and diethylenetriaminepentaacetic acid (DTPA),  - that no optical brighteners are used for product manufacture and refinement,  - that additional demand for fibres is only met with virgin fibres that are manufactured without using any optical brighteners, chlorine and halogenated bleaching chemicals. |  |
| **3.9** | - that the origin of the wood for the virgin fibres used can be verified,  Manufacturer of virgin fibres:  1.  2.  3.  Origin of the timber used:  1.  2.  3.  Certification system(s) used:  1.  2.  3.  - that the respective COC (Chain of Custody) certificates are attached, |  |
| **3.10** | - that the products under paragraph 2 do not contain any ingredients that would require the labelling of the product in accordance with the German Ordinance on Hazardous Substances, |  |
| **3.11** | – that the following information (or words to that effect) appears on the packaging of the product: „Painted woodchip wallpaper and used wallpaper can be disposed of with your residual (non-recyclable) household waste.“ |  |

**Annexes**

* Test protocol according to para. 3.3 (every second year)
* Annex 6, Parts I and II, to the Contract
* Declaration from the colorant supplier according to paras. 3.5, 3.6 and 3.7  
  (Annexes 2 **and** 3 to the Contract pursuant to DE-UZ 35)
* Declaration fro the Supplier according to para. 3.07   
  (Annex 3 to the Contract pursuant to DE-UZ 35)

Place:       Applicant

(Authorized signature and

Date:       company stamp)