|  |  |  |
| --- | --- | --- |
| **Annex to the Contract pursuant to DE-UZ 76**  **Blue Angel Eco-label for**  **„Low-Emission Panel-Shaped Materials**  **(Construction and Furnishing Panels)**  **for Interior Construction“** |  | **Please use this**  **form !** |

Manufacturer (Applicant):

Distributor (Label user):

Brand / trade name[[1]](#footnote-1)

Product designation:

DIN EN:

**Statement by the Applicant:**

| **Paragraph** | **Declarations / Compliance Verifications** | **Yes** | **No** |
| --- | --- | --- | --- |
| 3.1 | **General Requirements**  The legal provisions of the European and German chemicals legislation, above all REACH Regulation Annexes XIV and XVII, POP Regulation Annex I, GefStoffV (Ordinance on Hazardous Substances), 25th BImSchV (25th Federal Immission Protection Ordinance) and the CLP Regulation are complied with. |  |  |
| Attached hereto is the applicant's declaration:  **Annex 4 - form** |  |  |
| Attached hereto are the Technical Data Sheets and the Material Safety Data Sheets of the constituents **TDS/MSDS** |  |  |
| 3.2 | **Manufacture**  Are the panels wood-based? |  | **Go to 3.2.2** |
| 3.2.1 | **Requirements for the Timber**  All timber processed comes from legal sources under Regulation (EU) No 995/2010. |  |  |
| At least 70 percent of the wood used for wood-based materials comes from sustainably managed forests. |  |  |
| Attached hereto is a record of the wood used:  **Annex 2 - form** |  |  |
| Options to verify the use of timber from sustainable forestry:  ● Attached hereto is a certificate from the raw material supplier certifying a chain of custody (CoC) according to the FSC or PEFC criteria:  **FSC or PEFC Certificate**  and / or  ● Attached hereto are other appropriate compliance verifications according to Appendix 1:  **Annex 3 - form** |  |  |
| 3.2.2 | **Boards from expanded glass**  The mineral content of boards from expanded glass granulate is at least 90 % (w/w).  The expanded glass granulate used for production of the board is made of at least 90 % (w/w) recycled glass.  Bisphenole A was not detected (detection limit 0,1 mg/kg).  **Test report** |  |  |
| 3.2.3 | **Life Cycle Assessment (LCA) Parameters**  Parameters regarding GWP, ODP, AP, EP, POCP as well as primary energy are published on the basis of DIN EN 15804. |  |  |
| ● Attached hereto is a current Environmental Product Declaration **EPD**  Or  ● Attached hereto is another comprehensible verification document  **Data pursuant to DIN 15804** |  |  |
| 3.3.1 | **Indoor Air Quality**  Attached hereto is the test report: **Test report** |  |  |
| 3.3.2 | **Emission from boards made of expanded glass**  The board does not emit Bisphenole A at 60°C (detection limit 0,5 µg/m³)  **Test report** |  |  |
| 3.3.3 | **Odour Test (optional)**  Attached hereto is a test report according to DIN ISO 16000-28:  **Test report** |  |  |
| 3.3.4 | **Fitness for Use**  The product meets the usual quality requirements for fitness for use, especially the relevant DIN or CEN standards (cf. para. 2). |  |  |
| 3.3.5 | **Notes**  Information on how to obtain the technical Data Sheet is provided on the product and the Technical Data Sheet is made available on the Internet. |  |  |
| 3.4  3.4.1 | **Recycling and Disposal**  **Halogens**  No halogenated organic compounds are used in the manufacture of the composite panels.  In the case of detection: the concentration of the halogens fluorine, chlorine and bromine is determined by means of combustion analysis (total digestion) and does not exceed 1g/kg as content of tolerable impurities. **Test report** |  |  |
| 3.4.2 | **Flame Retardants**  Flame retardants are used.  If **YES**, these are inorganic ammonium phosphates (diammonium phosphate, ammonium polyphosphate etc.), other dehydrating minerals (aluminium hydroxide or the like), or expandable graphite. |  |  |
| 3.4.3 | **Biocides**  Biocides are not used; this requirement exempts biocides exclusively used for in-can preservation in aqueous coating materials. |  |  |
| 3.5 | **Consumer Information**  The consumer information including (minimum) information according to para. 3.5 is attached hereto and made available on the Internet:  **Consumer Information** |  |  |

Place:       Applicant:

(Authorized signature

Date:       and company stamp)

1. One Annex to the Contract is to be completed for each different product. [↑](#footnote-ref-1)